Test ID: 	G4-215#2306	Ring: 	R2B14(2199)	
Positive Dir: 	Down	Calibration: 	Auto (2141)	
Location: 	Flange -6"	Version: 	3.105, Wavemaker G4-215	
OutputVpp: 	200	Protocol: 	R2B - Standard Sequence	
Size: 	14 inch	GPS: 	42°1.0718'N, 87°55.3588'W	
Tested: 	Jan 28 2015 10:30	Client: 	GTI - Test Spool	
Tested by: 	Peter Rosencranz [TEAM]	Procedure: 	UT.GUL.4 R0	
Verified by: 		DACs: 	Call=5%, Weld=23%	
AvgSNR (dB): 	47.5	MaxSNR (dB): 	50.7	

General Notes: 	GTI -  (B-Side/South Riser)
14" Test spool - Test 1 16 averages
Positive direction is Down 
No visible corrosion noted at test site
Test spool is wrapped in 1mm plastic wrap.
UT-T @ Test Site: E-0.363" S-0.364" W-0.365" N-0.364"	

Feature	Location	Length	Class	Notes	
-F1	-0'4"	~	End	End of diagnostic test range. 	
-F2	-0'6"	0	Flange	Location of a blind flange  - Visually verified.	
+F1	0'6"	0	Mirror	False echo/Phantom signal - Mirror of Flange (-F1) in the Negative (Up) direction.	
+F2	2'7"	0	Bend	Location of a 90 degree elbow that bends to the Northwest.	
+F3	2'10"	~	Wrapping	Well adhered protective wrap (approx. 1mm thick) begins on the test spool and extends into the buried section.	
+F4	3'1"	0.416687	Medium	Area of MEDIUM concern at the 7 o'clock (Bottom Southwest) position on the test spool - Reduced sensitivity at this location due to amplitude diminishing nearfield effects.	
+F5	4'1"	0.5	Severe	Area od MAJOR concern at the 6 o'clock (Bottom) position on the test spool. Localized indication with a peak CSC of ~10%	
+F6	5'4"	1.2	Anomaly	Anomalous area of concern - Atypical weld reflection identified on the horizontal length of the 90 degree elbow.	
+F7	7'1"	0.33335	Minor	Area of MINOR concern at the 4 o'clock (Bottom Northeast) position on the test spool - Localized indication with a peak CSC of ~4%	
+F8	7'7"	1.00005	Minor	Area of MINOR concern - probable generalized corrosion along this length of the test spool with a peak CSC of ~4%.	
+F9	8'8"	0	Medium	Area of MEDIUM concern at the 9 o'clock (Southwest) position on the test spool with a peak CSC of ~5%	
+F10	8'10"	0.250012	Minor	Area of MINOR concern at the 9 o'clock (Southwest) position on the test spool with a peak CSC of ~3%	
+F11	8'11"	~	Earth	Test spool enters earth from the South side of the buried section.	
+F12	9'3"	0	Anomaly	Anomalous area - unquantifiable reflection possibly associated with deviations/voids in the protective coating and/or corrosion/defects at this location.	
+F13	9'8"	0.666699	Medium	 Area of MEDIUM concern at the 3 o'clock (Northeast), 6 o'clock (Bottom), & 11 o'clock (Top Southwest) positions on the test spool with a peak CSC of ~7%	
+F14	10'11"	0	Anomaly	Anomalous area - unquantifiable reflection possibly associated with deviations/voids in the protective coating and/or corrosion/defects at this location.	
+F15	11'5"	0	Medium	Area of MEDIUM concern at the 7 o'clock (Bottom Southwest) position on the test spool with a peak CSC of ~5%	
+F16	11'9"	0.5	Severe	Area of MAJOR concern (Very localized indication) at the 7 o'clock (Bottom Southwest) position on the test spool with a peak CSC of ~4%. 	
+F17	12'8"	0	Minor	Area of MINOR concern at the 4 o'clock (Bottom Northeast) position on the test spool  with a peak CSC of ~3%	
+F18	13'5"	0.5	Anomaly	Anomalous area - unquantifiable reflection possibly associated with deviations/voids in the protective coating and/or corrosion/defects at this location.	
+F19	15'7"	0.250012	Minor	Area of MINOR concern at the 4 o'clock (Bottom Northeast) position on the test spool  with a peak CSC of ~4%	
+F20	16'5"	0	Medium	Area of MEDIUM concern at the 2 o'clock (Top Northeast) position on the test spool - Localized indication with a peak CSC of ~6%	
+F21	17'5"	0.5	Anomaly	Anomalous area - unquantifiable reflection possibly associated with deviations/voids in the protective coating and/or corrosion/defects at this location.	
+F22	17'11"	0	Severe	Area of MAJOR concern (Very localized indication) at the 5 o'clock (Bottom Northeast) position on the test spool  with a peak CSC of ~5%	
+F23	18'5"	0.500024	Medium	 Area of MEDIUM concern at the 1 o'clock (Top Northeast), 5 o'clock (Bottom Northeast), & 11 o'clock (Top Southwest) positions on the test spool with a peak CSC of ~9.5%	
+F24	19'1"	~	End	End of diagnostic test range.