Test ID: 	G4-216#1069	Ring: 	R2F03(2303)	
Positive Dir: 	Unspecified	Calibration: 	Auto (320)	
Location: 	Support -6'5"	Version: 	3.102, Wavemaker G4-216	
Size: 	3 inch (.216")	GPS: 	38°50.2405'N, 90°3.6958'W	
Tested: 	Mar 23 2012 08:20	Client: 	Conoco Phillips	
Tested by: 	Andrew Mccracken [TEAM]	Procedure: 	UT.GUL.1 R0	
Verified by: 	Mike Sternik [TEAM]	DACs: 	Call=5%, Weld=23%, F=100%	
Protocol: 	R2F - Default Sequence	OutputVpp: 	200	

General Notes: 	3" #1 Prefactionary Tops To P-13 B27734
Pipe is not insulated at test location 
Positive Direction is West 
No corrosion at test collar 
Line is not live blinded due to leak 
Line is not painted 
UT Readings:
 Top: 0.197" North: 0.226" South: 0.220" Bottom: 0.194"	

Feature	Location	ECL	Length	Extent	Class	Notes	
-F6	-15'5"	-	0	90	Flange		
-F5	-12'9"	6	0	60	Minor	Pit gauge readings were 0.0625" around entire pipe in this area. Unable to get UT readings at area.	
-F4	-7'8"	7	0	50	Minor	Pit readings of 0.0625" noted generally around entire pipe in this area. UT readings Top:0.209" North:0.236" South:0.230" Bottom:0.210"	
-F3	-6'5"	-	0	25	Support		
-F2	-6'4"	5	0	25	Minor	Unable to get UT and pit gauge readings due to surface conditions. 	
-F1	-3'0"	4	2	12	Minor	Pit Readings of 0.0625" to 0.1875" noted at top of pipe. UT readings where areas allowed was Top:0.206" North:0.233" South:0.232" Bottom:0.233". 	
+F1	6'2"	-	0	3	Other	Steam Trace Band	
+F2	6'7"	-	0	80	Other	Steam Trace Band	
+F3	7'0"	-	0	90	Weld	Shop Weld	
+F4	9'11"	-	0	0	Other	Steam Trace Band	
+F5	12'7"	-	0	70	Other	Steam Trace Band	
+F6	15'4"	-	0	0	Other	Steam Trace Band	
+F7	18'6"	-	0	0	Other	Steam Trace Band	
+F8	21'10"	-	0	0	Other	Steam Trace Band	
+F9	23'7"	-	0	60	Support		
+F10	28'3"	-	0	0	Other	Steam Trace Band	
+F11	29'7"	-	0	100	Other	Steam Trace Band	
+F12	30'0"	-	0	100	Weld		
+F13	31'2"	-	0	70	Other	Steam Trace Band	
+F14	31'6"	-	0	90	Other	Steam Trace Band	
+F15	38'10"	-	0	90	Support		
+F16	52'10"	-	0	100	Weld	Shop Weld	
+F17	53'9"	-	0	80	Support		
+F18	57'9"	-	0	0	Other	Steam Trace Band	
+F19	59'11"	-	0	0	Other	Steam Trace Band	
+F20	67'9"	-	0	25	Other	Steam Trace Band	
+F21	68'9"	-	0	80	Support		
+F22	75'0"	-	0	100	Weld		
+F23	83'9"	-	0	80	Support		
+F24	84'1"	-	0	80	Other	Steam Trace Band	
+F25	90'3"	-	0	10	Other	Steam Trace Band	
+F26	92'0"	-	0	80	Other	Steam Trace Band	
+F27	95'10"	-	0	30	Other		
+F28	97'11"	-	0	100	Weld	Shop Weld	
+F29	98'7"	-	0	90	Support		
+F30	113'7"	-	0	50	Support		
+F31	120'1"	-	0	100	Weld		
+F32	128'7"	-	0	45	Support		
+F33	142'11"	-	0	90	Weld		
+F34	143'7"	-	0	90	Support		
+F35	158'7"	-	0	60	Support		
+F36	163'4"	-	~		End		
+F37	166'1"	-	0	100	Weld		
+F38	188'7"	-	0	100	Weld		
+F39	211'9"	-	0	100	Weld